# XTUV Command-line Parameters

The following table describes the command-line parameters for `XTUV`.

XTUV Command-Line Parameters
Command | Description
--- | ---
XTUV | Displays real-time CICS RED counters and other information.
XTUV,command,PRINT | Displays the details on any command and prints the output to CEEOUT.
XTUV,DUMP,hex-address,length | Displays the details of a specific address storage for diagnostic information.
XTUV,DUMP,CICS | Displays the TSQ main storage.
XTUV,DUMP,RED | Displays RED main storage
XTUV,DUMP,REC | Displays RED Receiver Storage.
XTUV,DUMP,TRG | Displays RED Trigger storage.
XTUV,ERR,# | Displays the details of an error record. Note: The hash sign (#) is the record number of an error in the error queue.
XTUV,ERR,DELETE | Displays the details of the first error record from the error queue and then deletes the record from the queue.
XTUV,ERR,PURGE | Deletes all the records from the error queue.
XTUV,HELP|? | Lists all the keywords for the available commands.
XTUV,REAL|RT | Displays real-time CICS RED counters and other information.
XTUV,REC | Displays RED CICS receiver storage information.
XTUV,RED | Displays the RED main storage.
XTUV,STATS,<url> | Displays the RED statistics for CICS Listener.
XTUV,TRG[,NEXT][,#] | Displays all the pools and members established by the Substation ES RED interface. Optional operand NEXT page or NEXT,# to next # of interface. Where # is the number 1 to 6 interface.

Copyright © TIBCO Software Inc. All rights reserved.