# Mainframe Logger Parameters

The Mainframe Logger member specifies the parameters for Substation ES Log and Trace Agents can write recorded information to z/OS System Logger Stream. The interface member template is stored in TIBSLOG in the USERHLQ.PARM data set.

If you make a copy of this member, you can point to it by specifying the member name on the SYSLOG-MEM keyword in the main SSP parameter member.

For more information about the Mainframe Logger usages, refer to the TIBCO Mainframe Logger User's Guide.

The following table lists the Mainframe Logger parameters supported by Substation ES.

Mainframe Logger Parameters
Parameter | Description
--- | ---
LOGSTREAM-ID = {name} | Optional The LOGSTREAM-ID parameter specifies the System Logger Stream name, which will contain the log of Substation ES messages, errors, and general information. The records can be displayed by the System Logger Stream Data Viewer. It can contain upto 26 alphanumeric characters.
STATISTICS = {N | Yes, No} | Optional The STATISTICS parameter specifies whether Substation ES statistics recording indicator is Yes or No. The default value is No.
STSSTREAM-ID = { name} | Optional The STSSTREAM-ID parameter specifies the System Logger Stream name, which will contain the Substation ES statistics information. The records can be display by the System Logger Stream Data Viewer. It can contain upto 26 alphanumeric characters.
TRCSTREAM-ID = {name} | Optional The TRCSTREAM-ID parameter specifies the System Logger Stream name, which will contain the trace of Substation ES messages, errors, and general information. The records can be display by the System Logger Stream Data Viewer. It can contain upto 26 alphanumeric characters.

Copyright © TIBCO Software Inc. All rights reserved.