# SXTH Command-line Parameters

The following table describes the command-line parameters for `SXTH`.

Command | Description
--- | ---
SXTH | Displays a statistics summary for the Substation ES CICS interface queue resources.
SXTH,ALL | Displays a statistics summary for the Substation ES CICS interface queue resources.
SXTH,DEF | Displays the default information of the Substation ES CICS interface queue resources.
SXTH,ERR | Displays the details on the first error record from the error queue.
SXTH,ERR,DELETE | Displays the details on the first error record from the error queue and then deletes the record from the queue.
SXTH,ERR,PURGE | Deletes all the records from the error queue.
SXTH,HELP-? | Lists all the keywords for the available commands.
SXTH,HVT | Displays the concurrent activity of the HVT queues.
SXTH,TSQ | Displays the concurrent activity of the HV TSQ triggers.
SXTH,PTDQ,TDQ Name,start record,number of records | Reads the TDQ records from the specified Transient Data Queue and produces a hex format printout of the queue record. Directs the output to `CEEMSG` of the CICS region.
SXTH,PTSQ,TSQ Name,start record, number of records | Reads the TSQ records from the specified TSQ and produces a hex format printout of the queue record. Directs the output to `CEEMSG` of the CICS region.
SXTH,QUE | Displays the usage information on the default Trigger Queue.
SXTH,QUE,TDQ Name | Displays the queue usage information on the given TD queue name.
SXTH,TRG | Displays the concurrent active statistics for the triggers and CICS initiated request or reply processes.
SXTH,VER | Displays the date and timestamp of the module compiled.

Copyright © TIBCO Software Inc. All rights reserved.