# Transformer Configuration Panel

The Transformer Configuration panel provides options for defining a new set of conversion records or for working with an existing set of conversion records.

## Panel Layout

    SXTPMAIN ------------- TIBCO Substation (ES) with RED V1 --------------------
                          Transformer Configuration 2.9
     SELECT OPTION  ===>

     File Name ===> USERHLQ.DATASET
     Read Only ===> N (Yes/No)
     Debug     ===> 0 (0 - 5)

     Select One of the Following:
       1 - Define Message Contents
       2 - Define Buffer Areas
       3 - Define Conversion Relationships
       4 - Define Processing System Resources
       5 - Define ESB Endpoints and Parameters
       6 - Define Recipes - Inbound/Outbound/Destinations/BES
       7 - Define Triggers - Outbound Convert/Destinations
       8 - Define Groups
       9 - Show Related Structures
      10 - COBOL Copybook Converter

     Enter END command to terminate.

## Field Description

The following table lists the fields in the Transformer Configuration panel:

Field | Description
--- | ---
SELECT OPTION | You can select the panels and functions to perform through the Transformer DCUI panels. The following options are available: 1 - Define Message Contents 2 - Define Buffer Areas 3 - Define Conversion Relationships 4 - Define Processing System Resources 5 - Define ESB Endpoints and Parameters 6 - Define Recipes – Inbound/Outbound/Destinations/BES 7 - Define Triggers – Outbound Convert/Destinations 8 - Define Groups 9 - Show Related Structures 10 - COBOL Copybook Converter
File Name | The name of the Substation ES Transformer configuration VSAM file. You must specify the file name before selecting an option.
Read Only | If you select N, updates made to the Transformer configuration VSAM file are saved. If you select Y, the updates are not saved. Valid selections: Y(es) and N(o). Default selection: N.
Debug | Required. The level of informational messages recorded to the screen. This value must be 0 unless TIBCO Support require the change. Valid values: 0 - 5. Default value: 0.

Copyright © TIBCO Software Inc. All rights reserved.