# Administration Interface Parameters

The administration interface member is SXSIADM, which you can access by performing a standard TSO edit. If you make a copy of this member, you can point to it by specifying the member name on the INTF-MEMBER keyword in the main SIP definition member. The following table lists the administration interface parameters supported by Substation ES.

Administration Interface Parameters
Parameter | Description
--- | ---
DESCR = {description} | See DESCR = {description} under "Common Initialization Parameters" above.
ESB-INTF-ID = {identifier} | The ESB-INTF-ID parameter specifies the identifier of the Substation ES ESB Interface. This interface publishes the heartbeat trigger message initiated from Substation ES. The installation default value is ESB01.
HEARTBEAT-COMMAND = {COMMAND} | The HEARTBEAT-COMMAND parameter specifies the CONSOLE command that the heartbeat trigger message publishes. In one admin interface, you can include this parameter a maximum of 5 times. The default command is SHOW,INTF.
HEARTBEAT-INTERVAL = {number} | The HEARTBEAT-INTERVAL parameter specifies the heartbeat trigger message publication rate. If the interval is greater than zero, the heartbeat starts. The valid range is from 2 to 300 seconds. The value of 0 stops the heartbeat trigger service.
HEARTBEAT-SERVICE = {name} | The HEARTBEAT-SERVICE parameter specifies the trigger service name to be used for the heartbeat message. This must match a corresponding Trigger service definition defined in the configuration file. The installation default value is HEARTBEAT.
INTF-ID = {name} | See INTF-ID = {name} under "Common Initialization Parameters" above.
INTF-TYPE = {number} | See INTF-TYPE = {number} under "Common Initialization Parameters" above.
LOG-REMOTE = {N | Yes, No} | The LOG-REMOTE parameter specifies whether to log remote operational commands to the Substation log file. The default value is N, indicating that remote operational commands are not logged.
MODULE-NAME = {TIBSSADM | name} | The MODULE-NAME parameter specifies the name of the Administration interface load module. If no name is specified, the default load module name TIBSSADM is used.
START-YN = {N | Yes, No} | See START-YN = {Yes, No} under "Common Initialization Parameters" above.
TRCLVL-OPS = {0 | 0-5} | (Optional) The TRCLVL-OPS parameter specifies the trace level of the messages produced for a Substation ES operational command. This parameter is mainly for debugging, with most of the information written to the trace file.
WORKERS = {3 | number} | The WORKERS parameter specifies the number of concurrent internal threads that service Substation ES administration performance. The valid values range from 1 through 30. The default value is 3.

Copyright © TIBCO Software Inc. All rights reserved.