# JCL Sample (SXSCFC26)

Execution is controlled by `parm` values and JCL statements.

    //EXPORT  EXEC PGM=SXT3CV26,REGION=0M,PARM='parm values'
    //STEPLIB   DD DISP=SHR,DSN=< USERHLQ>.LOAD
    //TIBLOG    DD SYSOUT=*
    //SYSPRINT  DD SYSOUT=*
    //SYSOUT    DD SYSOUT=*
    //CEEDUMP   DD SYSOUT=*
    //SYSUDUMP  DD SYSOUT=*
    //CONFIG    DD DISP=SHR,DSN=old.config.file
    //EXPORT    DD DISP=(,CATLG),DSN=new.export.file,
    //             UNIT=SYSDA,SPACE=(TRK,(20,20)),
    //             DCB=(BLKSIZE=14000.LRECL=350,RECFM=VB)

The following table shows Configuration File Conversion Utility DDNames:

DDNAME | Description
--- | ---
CONFIG | Points to the old Transformer Configuration file that provides the input data to the conversion process.
EXPORT | Points to a new EXPORT file that is written during an export operation.

Copyright © TIBCO Software Inc. All rights reserved.