# HVT Trigger Transactions

The following table shows the command-line parameters for sample HVT tasks.

SXTF and SXT6 Command-Line Parameters
Command | Description
--- | ---
SXTF/SXT6 | Sends one message through HVT in IVP format.
SXTF/SXT6,HELP-? | Lists all the keywords for the available commands.
SXTF/SXT6,type(G|R|O|S),number_of_records | Sends multiple IVP trigger messages through HVT in type. The valid type values are `G` for Guaranteed, `R` for Reliable, `O` for Ordered, and `S` for Temporary Storage Trigger.
SXTF/SXT6,type(G|R|O|S),number_of_records,data_length(1 - 4096000) | Sends multiple messages through HVT in type and data_length. The valid type values are `G` for Guaranteed, `R` for Reliable, `O` for Ordered, and `S` for Temporary Storage Trigger. The maximum data length for the TSQ Trigger is 32000.
SXTF/SXT6,type(G|R|O|S),number_of_records,data_length(1 - 4096000),service_name | Sends multiple messages through HVT in type and data_length to service_name (the trigger identifier). The valid type values are `G` for Guaranteed, `R` for Reliable, `O` for Ordered, and `S` for Temporary Storage Trigger. The maximum data length for the TSQ Trigger is 32000.
SXTF/SXT6,Type(G|R|O|S),number_of_records,data_length(1 - 4096000),service_name,CTN | Sends multiple messages through HVT in type and data_length to service_name (the trigger identifier), using CTN number of containers. The valid type values are `G` for Guaranteed, `R` for Reliable, `O` for Ordered, and `S` for Temporary Storage Trigger. The maximum data length for the TSQ Trigger is 32000. The valid range for CTN is 1 to 20.
SXTF,Type(G|R|O|S),number_of_records,data_length(1 - 4096000),service_name,CTN, delay_in_seconds SXT6,Type(G|R|O|S),number_of_records,data_length(1 - 4096000),service_name,CTN, delay_in_seconds .01,#Tasks | Sends multiple messages through HVT in type and data_length to `service_name` (the trigger identifier), using CTN number of containers, and with a delay of delay in seconds between calls to `SXCQWRIT` or `SXCQWTSQ`. The valid type values are `G` for Guaranteed, `R` for Reliable, `O` for Ordered, and `S` for Temporary Storage Trigger. The maximum data length for the TSQ Trigger is 32000. The valid range for CTN is 1 to 20.

The messages sent are either the default IVP messages or, if data_length is specified, a record of length data_length filled with 1--------10--------20------.

Copyright © TIBCO Software Inc. All rights reserved.