# Additional Configuration

You can use Substation ES to specify different interface configurations to meet various business requirements.

For example, you can configure a single Substation ES instance to simultaneously communicate with multiple CICS regions. Alternatively, you can configure multiple Substation ES instances to communicate with the same CICS region. The configuration choice depends on your system requirements.

Copyright © TIBCO Software Inc. All rights reserved.