# Configuration File Utility Messages

The following table describes the messages for the configuration file utility.

Code | Description
--- | ---
`SXT7001I` | Utility departing, rc=RC
Explanation: The program has completed. System Action: Processing terminates.
`SXT7002E` | Invalid parm (no dash) Field
Explanation: The `parm` field is not preceded by a dash. User Response: Correct and resubmit. System Action: The utility terminates.
`SXT7003E` | Invalid parm Parm
Explanation: The value in the Parm field is invalid. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7004I` | Parms: Parm
Explanation: This message displays the runtime parameters. System Action: Processing continues.
`SXT7005E` | LDS error Err-Desc in Req-Desc
Explanation: The error as described occurred during the processing of a Linear Data Set request. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7006E` | Invalid call to LDS ERROR
Explanation: The call to the Linear Data Set access routine that defines the error communication has failed. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7007E` | Not a config file, cannot init
Explanation: The configuration file is not properly initialized and the permission to initialize it is withheld. User Response: Examine the configuration file and enable the program to initialize it, if desired. System Action: Processing terminates.
`SXT7008I` | Primary file opened Mode
Explanation: The configuration file is opened for either update or read-only. System Action: Processing continues.
`SXT7009E` | Invalid call to LDS-OUT ERROR
Explanation: The call to the Linear Data Set access routine that defines the error communication has failed. User Response: Contact TIBCO Support System Action: Processing terminates.
`SXT7010I` | Output (Compressed) file opened
Explanation: The secondary configuration file has successfully opened. System Action: Processing continues.
`SXT7011I` | Offending type is Type - Block
Explanation: This message shows the type of the invalid block. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7012C` | Invalid type code Num
Explanation: The`Verify_Chain` routine has detected an internal error. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7013E` | Deleted block in chain
Explanation: An internal structural error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7014E` | Invalid Identifier
Explanation: An internal structural error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7015W` | Missing BlockType in Chained from type of block
Explanation: A chain of blocks contains no entries. User Response: If this message refers to groups or back-end systems, the situation could well be valid. All other types of blocks must have entries. System Action: Processing continues.
`SXT7015E` | cfut Missing Information
Explanation: An internal structural error is in the configuration file. At least one recipe and trigger must exist. User Response: Correct the required definition. System Action: Processing terminates.
`SXT7016I` | Validation started
Explanation: The validation process has started. System Action: Processing continues.
`SXT7017E` | Recipe R-Name (BES) invalid BES
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7018E` | Recipe R-Name (T-Id) invalid Transport
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7019E` | Recipe R-Name (Input) invalid input Convert
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7020E` | Recipe R-Name (Output) invalid output Convert
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7022E` | Trigger T-Name (T-Id) invalid Transport
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7023E` | Trigger T-Name (Output) invalid output Convert
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7024E` | Buffer Id missing for Converter CnvtId (Address)
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7025E` | Msg Id missing for Converter CnvtId (Address)
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7026E` | Convert CnvtId Converter Address missing
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7027E` | Convert CnvtId RV-field FldName missing
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7028I` | Validate complete
Explanation: The validation process has completed. System Action: Processing continues.
`SXT7029I` | Import started
Explanation: The import process has begun. System Action: Processing continues.
`SXT7030W` | Import open error RC
Explanation: The import file has failed to open. User Response: See the previous message. System Action: Processing terminates.
`SXT7031W` | Import error RC
Explanation: The import process failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7032W` | Import close error RC
Explanation: The import file has failed to close. User Response: See the previous message. System Action: Processing terminates.
`SXT7033I` | Import completed
Explanation: The import process has completed successfully. System Action: Processing continues.
`SXT7034I` | Export started
Explanation: The export process has begun. System Action: Processing continues.
`SXT7035W` | Export open error RC
Explanation: The export process experienced an error while opening the output file. User Response: See the previous messages. System Action: Processing terminates.
`SXT7036I` | Export open successful
Explanation: The export output file has opened. System Action: Processing continues.
`SXT7037I` | Messages exported
Explanation: The related message definitions have been exported successfully. System Action: Processing continues.
`SXT7038I` | Buffers exported
Explanation: The related buffer definitions have been exported successfully. System Action: Processing continues.
`SXT7039I` | Convert Rules exported
Explanation: The definitions of the related conversion rules have been exported successfully. System Action: Processing continues.
`SXT7040I` | Backend Systems exported
Explanation: The related back-end system definitions have been exported successfully. System Action: Processing continues.
`SXT7041I` | Transports exported
Explanation: The related transport definitions have been exported successfully. System Action: Processing continues.
`SXT7042I` | Recipes exported
Explanation: The related recipe definitions have been exported successfully. System Action: Processing continues.
`SXT7043I` | Triggers exported
Explanation: The related trigger definitions have been exported successfully. System Action: Processing continues.
`SXT7044I` | Groups exported
Explanation: The related group definitions have been exported successfully. System Action: Processing continues.
`SXT7045W` | Export failed
Explanation: The export process has failed. User Response: See the previous messages. System Action: Processing terminates.
`SXT7046W` | Export close error RC
Explanation: Closing of the export process has encountered an error. User Response: See the previous message System Action: Processing terminates.
`SXT7047I` | Export completed
Explanation: The export process is complete. System Action: Processing continues.
`SXT7048C` | Rechain called with Type type
Explanation: The `Rechain` function of `compress` has found an internal error. User Response: Call TIBCO Support. System Action: Processing terminates.
`SXT7049C` | Rechain old block missing
Explanation: The `Rechain` function of `compress` has found an internal error. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7050C` | Rechain new block missing
Explanation: The `Rechain` function of `compress` has found an internal error. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7051I` | Compress started
Explanation: The `compress` function has begun. System Action: Processing continues.
`SXT7052I` | Compress completed
Explanation: The `compress` function has completed. System Action: Processing continues.
`SXT7053I` | Print started
Explanation: The `print` function has started. System Action: Processing continues.
`SXT7054I` | Print completed
Explanation: The print function has completed. System Action: Processing continues.
`SXT7055I` | Control block sizes:Num
Explanation: The control block sizes are Num. System Action: Processing continues.
`SXT7056I` | Hex Display complete
Explanation: The hex display function has completed. System Action: Processing completes.
`SXT7058I` | Initialized
Explanation: The utility has completed its initialization process. System Action: Processing continues.
`SXT7059W` | Remaining functions not executed
Explanation: The validate function has failed, causing a skipping of further processing. User Response: Correct the previous errors. System Action: Processing terminates.
`SXT7060W` | import or export init failed
Explanation: The `import` or `export` support initialization routines have failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7061W` | Export failed - rc= RC
Explanation: The `export` support routines have failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7062W` | Import failed - rc= RC
Explanation: The `import` support routines have failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7063W` | Compress failed - rc=RC
Explanation: The `compress` function has failed. User Response: See the previous messages for an explanation of the failure. System Action: Processing terminates.
`SXT7064W` | import or export term failed
Explanation: The `import` or `export` termination support routines have failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7065W` | Print incomplete - rc = RC
Explanation: The print function has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7066W` | Hex Dump incomplete - rc = RC
Explanation: The hex display function has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7067E` | Close of Config files failed
Explanation: An error occurred during the closing process of the configuration files. User Response: See the previous message. System Action: Processing terminates.
`SXT7068E` | No storage for parms
Explanation: The initial `malloc` job has failed. User Response: Increase the size of the region allocated for the job. System Action: Processing terminates.
`SXT7069W` | Primary set/reset to empty
Explanation: The primary configuration file has been set to empty. System Action: Processing continues.
`SXT7070I` | File SAVE successful
Explanation: All updates have been successfully recorded in the configuration file. System Action: Processing continues.
`SXT7071I` | Compressed file SAVE successful
Explanation: All updates have been successfully recorded in the secondary configuration file. System Action: Processing continues.
`SXT7072W` | No request given
Explanation: No action request is in the `parm` field. User Response: Accept the default. System Action: Processing continues. See message SXT7075I.
`SXT7074I` | Contents in hex follow:
Explanation: The hex display function has started. System Action: Processing continues.
`SXT7075I` | Default to -P (Print)
Explanation: No action request is in the `parm` field. User Response: Accept the default. System Action: Processing defaults to `Print.`
`SXT7076E` | Duplicate id Id in two Type blocks
Explanation: The same identifier is in two blocks of type Type. User Response: Correct the duplication with the update facilities. System Action: Processing continues.
`SXT7077I` | Import failed, rc=RC
Explanation: The import request has failed. User Response: See the previous messages. System Action: Processing terminates.
`SXT7078W` | Errors detected - terminating
Explanation: The previous errors have been found. User Response: See the previous messages. System Action: Processing terminates.
`SXT7079E` | Group Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7080E` | Recipe Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7081E` | Trigger Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7082E` | Transport Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7083E` | BackEnd Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7084E` | Converter Id has trailing blank
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7085E` | Convert Id buf-field FieldName missing
Explanation: An internal error is in the configuration file. User Response: Correct the configuration file. System Action: Processing continues.
`SXT7086W` | Compress cvt table error RC
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7087W` | Compress Table startup error RC
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7088W` | Compress Table Add error RC
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7089W` | Compress Table FIRST error RC
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7090W` | Compress Table Rechain from Table
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7091W` | Compress Table GET error RC
Explanation: An internal error occurred during the compress process. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7092E` | Convert Id RV-field FieldName wrong type
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7093E` | Convert Id RV-field FieldName wrong type
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7094E` | Convert Id Bffield not Null
Explanation: An internal error is in the configuration file. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7101I` | Utility arriving, Version Number - Date Time
Explanation: The utility has started. System Action: Processing continues.
`SXT7102I` | Input parms
Explanation: This message shows the input parameters. System Action: Processing continues.
`SXT7103I` | Anchor Block is origin
Explanation: The heading of a storage display shows the Anchor Block if a control block pointer is null. System Action: Processing continues.
`SXT7104I` | Origin Block
Explanation: The snap heading for the origin block of an invalid block is displayed if the origin pointer is not null. System Action: Processing continues.
`SXT7105I` | Block in error
Explanation: The snap heading of a control block is in error. System Action: Processing continues.
`SXT7106E` | Duplicate id Id in Type list ParentId
Explanation: ParentId identifies the message or buffer to which the duplicate IDs belong. User Response: Correct the configuration file. System Action: Processing continues.
`SXT7107I` | Table Error
Explanation: The snap heading of the error block has been returned by the table processor as part of error propagation. System Action: Processing continues.
`SXT7108I` | Table Add Error
Explanation: A conversion field has been added to an interim table, producing a table-related error. This is the snap heading of the table error block. System Action: Processing continues.
`SXT7109I` | Table FIRST Error
Explanation: The operation of repointing an interim table to its first entry has produced an error. This is the snap heading of the error block returned by the table processor. System Action: Processing continues.
`SXT7110I` | Table Rechain Error
Explanation: A table processing error occurred during an internal reorganization of a portion of the configuration file. This is the snap heading of a display of the error block returned by the table processor. System Action: Processing continues.
`SXT7111I` | Table GET Error
Explanation: A table processing error occurred during an internal reorganization of a portion of the configuration file. This is the snap heading of a display of the error block returned by the table processor. System Action: Processing continues.
`SXT7112I` | Snap of Type
Explanation: A snap display heading for all control blocks is shown as part of a request to show all entries in hex. System Action: Processing continues.
`SXT7113E` | Recipe Id missing BES, not MOI=9
Explanation: The recipe is missing a BES ID and is not MOI 9. User Response: Correct with the update facilities. System Action: Processing continues.
`SXT7114E` | Entry Id has no transport defined
Explanation: No transport is defined in the recipe or trigger ID. User Response: Correct with the update facilities. System Action: Processing continues.
`SXT7115E` | Entry Id reply method required out-conversion
Explanation: The recipe or trigger Id requires an output conversion specification, which is missing. User Response: Correct with the update facilities. System Action: Processing continues.
`SXT7116E` | Recipe Id missing input conversion
Explanation: An input conversion is not in the recipe Id. User Response: Correct with the update facilities. System Action: Processing continues.
`SXT7117E` | Recipe R-Name (addr) has wrong buffer bufid in Ext Prop
Explanation: The recipe R-Name at the location addr points to an invalid buffer identified as bufid in the Extension Properties section. User Response: Contact TIBCO Support. System Action: Validation continues.
`SXT7118E` | Recipe R-Name (addr) has inv buf fld in bufid in Ext Prop
Explanation: The recipe R-Name at the location addr points to an invalid buffer identified as bufid in the Extension Properties section. User Response: Contact TIBCO Support. System Action: Validation continues.
`SXT7119E` | Recipe R-Name (addr) has wrong buffer bufid in Ext MT
Explanation: The recipe R-Name at the location addr points to an invalid buffer identified as bufid in the Extension Multi-Task section. User Response: Contact TIBCO Support. System Action: Validation continues.
`SXT7120E` | Recipe R-Name (addr) has inv buf fld in bufid in Ext MT
Explanation: The recipe R-Name at the location addr points to an invalid buffer identified as bufid in the Extension Multi-Task section. User Response: Contact TIBCO Support. System Action: Validation continues.
`SXT7121E` | Not Proper Version - Want:Number1, File:Number2
Explanation: The configuration file has the wrong version number. The configuration file contains a Version Number, which is compared by the ISPF Configuration Panels and Substation ES to ensure that an incorrect configuration file is not used. Substation ES expects version Number1, while the current configuration file has version Number2. User Response: Convert the configuration file to the current Substation ES release version. For details, see the section on Migrating from Previous Releases in the TIBCO Substation ES Release Notes. System Action: ISPF Configuration Panels and Substation ES terminate.
`SXT7122W` | Option -T and -Z ignored with -C
Explanation: The options on running `SXT3FUT` contained `-T` and `-Z` and `-C`. However, the `-C` option is incompatible with `-T` and `-Z`; it cannot be used with either. System Action: Substation ES continues processing, using `-C` option. The `-T` and `-Z` options are ignored.
`SXT7210I` | Import/Export debug Num
Explanation: The `import` or `export` subroutine has initialized, with debug level Num. System Action: Processing continues.
`SXT7211I` | Config import or export Terminated
Explanation: The import or export process has completed. System Action: Processing continues.
`SXT7212C` | Type ProcType not I or O
Explanation: During initial processing of import or export, the type of process was invalid. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7213E` | Open failed for FileName because RSN
Explanation: Opening the import or export file failed. User Response: Ensure that the correct DD statement is in the JCL. System Action: Processing terminates.
`SXT7214I` | File name FileName, Mode= File Description
Explanation: This is the file name along with information on the data set. System Action: Processing continues.
`SXT7215I` | Import/export file opened type Type
Explanation: The import or export file has opened for the processing type I or O. System Action: Processing continues.
`SXT7216I` | Import end of input
Explanation: The entire import file has been read. System Action: Processing continues.
`SXT7217E` | Import read error Err:Description
Explanation: During the reading of the import file, an error other than end-of-file occurred. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7218I` | Closed Import/Export file, rc=RC
Explanation: The import or export file has closed with return code RC. System Action: Processing continues.
`SXT7219E` | Write error in export Err:Description
Explanation: During the writing of an export record, a system-related error occurred. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7220I` | Export type Num start Address
Explanation: The exported record is of the type Num and started from Address. System Action: Processing continues.
`SXT7221C` | Invalid type code Num - Id lookup
Explanation: An internal error has occurred. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7223I` | Import type Num state state
Explanation: This is the imported record type and state. System Action: Processing continues.
`SXT7224C` | bad type=Num to Delete_Unused
Explanation: An internal logic error occurred during the processing of Import. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7225E` | Import file sequence or content error
Explanation: A previous message describes in detail the sequence or content error that was found. User Response: Examine the source of the `import` file. System Action: Processing terminates.
`SXT7226E` | Import Field error RecordType record: Id field Name Not numeric
Explanation: During the processing of import, the field Name in the record Id of type RecordType was found to be not numeric. User Response: Correct the import record or the original configuration file from which the file was exported. System Action: Processing continues.
`SXT7227E` | Import Field error RecordType record: Id field Name Invalid value
Explanation: During the processing of import, the field Name in the record Id of type RecordType was found to have an invalid value. User Response: Correct the `Import` record or the original configuration file from which the file was exported. System Action: Processing continues.
`SXT7228E` | Import Field error RecordType record: Id field Name Cannot be a null value
Explanation: During the processing of import, the field Name in the record Id of type RecordType was found to have a null value. That field must have a nonnull value. User Response: Correct the import record or original configuration file from which the file was exported. System Action: Processing continues.
`SXT7229E` | Import Field error RecordType record: Id field Name Duplicate identifier
Explanation: During the processing of import, the field Name in the record Id of type RecordType was found to be a duplicate identifier. User Response: Correct the import record or the original configuration file from which the file was exported. System Action: Processing continues.
`SXT7230E` | Group Member out of sequence
Explanation: A Group Member record is received out of sequence. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7231E` | Invalid record type Type
Explanation: An unknown record type was read from the import file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7232E` | Excluded RVG block used: Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7234E` | Excluded BFL block used
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7235E` | RV Msg in use by Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7236E` | Buffer in use by Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7237E` | Buf Field Field-Id not exist in Identifier
Explanation: The specified buffer field does not exist in Identifier. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7238E` | RV Msg field Field-Id not exist in Identifier
Explanation: The specified message field does not exist in Identifier. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7239E` | Buffer in use by Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7240E` | Buffer not exist - Identifier
Explanation: The specified buffer does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7241E` | RV Msg not exist - Identifier
Explanation: The specified message record does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7242E` | Back End System used by Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7243E` | Convert-I not exist - Identifier
Explanation: The specified input conversion does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7244E` | Convert-O not exist - Identifier
Explanation: The specified output conversion does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7245E` | Backend not exist - Identifier
Explanation: The specified Backend system does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7246E` | Transport not exist - Identifier
Explanation: The specified transport does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7247E` | Convert-O not exist - Identifier
Explanation: The specified output conversion does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7249E` | Transport not exist - Identifier
Explanation: The specified transport does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7250E` | Transport used by Identifier
Explanation: A delete request from the import file specifies the block Identifier, but that block has already been used. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7251E` | Recipe or Trigger not exist - Identifier
Explanation: The specified recipe or trigger does not exist. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7252E` | Record identifier incorrect
Explanation: The input record is not an `Import` record. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7254E` | Table processing error in Function
Explanation: A table processing error occurred during the Function process. User Response: See the following message for a description of the error. System Action: Processing terminates.
`SXT7258E` | CV Rule for RVMSG missing - Identifier
Explanation: After the processing of an import file, certain entries were tabled for later resolution. One of those entries cannot be resolved. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7260E` | Premature End of File
Explanation: The import file has terminated without a trailer record. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7261E` | Imbedded header record
Explanation: A header record was read from the import file in other than the first position. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7262E` | Commit out of sequence
Explanation: A commit record was read from within a set of field records. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7264E` | Trailer out of sequence
Explanation: A trailer record was read from the import file from within a set of field records. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7265E` | RV fld had delete code
Explanation: A Rendezvous field record has the delete code set, which is not allowed. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7266E` | RV Field out of sequence
Explanation: The Rendezvous field record must be part of the list of Rendezvous field records. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7267E` | RV Message out of sequence
Explanation: The Rendezvous message record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7268E` | Buffer field has delete code
Explanation: A buffer field record has the `delete` code set, which is not allowed. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7269E` | Buffer field out of sequence
Explanation: The `Buffer` field record must be part of the list of buffer field records. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7271E` | Internal work malloc failed
Explanation: The storage is not adequate for a `malloc` request. User Response: Increase the region size and resubmit. System Action: Processing terminates.
`SXT7272E` | Buffer out of sequence
Explanation: The Buffer record cannot occur at the current position in the file. User Response: Correct the `Import` file and resubmit. System Action: Processing terminates.
`SXT7273E` | Conversion field has delete code
Explanation: A Conversion field record has the `delete` code set, which is not allowed. User Response: Correct the `Import` file and resubmit. System Action: Processing terminates.
`SXT7274E` | Conversion field out of sequence
Explanation: The Conversion field record cannot occur at the current position in the file. User Response: Correct the Import file and resubmit. System Action: Processing terminates.
`SXT7275E` | Conversion rule out of sequence
Explanation: The Conversion rule record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7276E` | Backend system out of sequence
Explanation: The Backend System record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7277E` | Recipe out of sequence
Explanation: The Recipe record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7278E` | Trigger out of sequence
Explanation: The Trigger record cannot occur at this position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7279E` | Transport out of sequence
Explanation: The Transport record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7280E` | Group out of sequence
Explanation: The Group record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7281E` | Group Pointer out of sequence
Explanation: The Group Pointer record cannot occur at the current position in the file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7282E` | Import field error: Type record: Id field Field-Id - Value too long
Explanation: The value of the field is too large to fit in the receiving field in the configuration file. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7283I` | Export Type: Identifier
Explanation: This message is issued for each record or group of records exported if `Verbose` is requested for the `export` operation. System Action: Processing continues.
`SXT7284E` | Null anchor for delete unused
Explanation: An internal error has been detected. User Response: Notify TIBCO Support. System Action: Processing terminates.
`SXT7287E` | Import field error: Type record: Id, field Field-Id - Invalid combination
Explanation: An invalid combination of field values has been found. Both fields are defined in Field-Id. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7288E` | Export type Type invalid
Explanation: The input record has an unrecognized type code. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7289E` | Export action Action invalid
Explanation: The input record has an unrecognized action code. User Response: Correct the import file and resubmit. System Action: Processing terminates.
`SXT7290E` | Extension out of sequence
Explanation: During the import process, an extension record was received out of sequence. User Response: Contact TIBCO Support. System Action: The import processing terminates.
`SXT7400I` | Selective Export arriving CompileTimeStamp
Explanation: The selective export utility has begun. System Action: Processing continues.
`SXT7402I` | Selective Export departing, rc=RC
Explanation: The selective export utility has terminated. System Action: Processing continues.
`SXT7410E` | No storage for parms
Explanation: A storage request failed. User Response: Increase the size of the `region` parameter and resubmit. System Action: Processing terminates.
`SXT7411E` | Invalid parm (no dash) Parm
Explanation: Parm is invalid because it is not preceded by a dash. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7412E` | Invalid parm Parm
Explanation: Parm is invalid. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7414I` | Parms: Parms
Explanation: All the input parameters are displayed. System Action: Processing continues.
`SXT7415E` | Error Code in LDS call for Request
Explanation: A request to the Linear Data Set has returned an error. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7416E` | Invalid call to LDS ERROR rc=RC
Explanation: A call to the LDS interface with error information has failed. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7417E` | Not a config file
Explanation: The configuration file defined in the JCL has not been properly initialized. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7418I` | Config file opened read-only
Explanation: The configuration file has been successfully opened. System Action: Processing continues.
`SXT7419E` | Open of ctl file failed
Explanation: The open request for the control file has failed. User Response: Correct the error and resubmit. System Action: Processing terminates.
`SXT7420I` | Open errno=Num - Description
Explanation: There are further details on message SXT7419E. User Response: See the previous message. System Action: Processing terminates.
`SXT7421I` | Open:DDName with OpenMode
Explanation: The control file has been successfully opened. System Action: Processing continues.
`SXT7422I` | End of File on controls
Explanation: All control statements have been read. System Action: Processing continues.
`SXT7423E` | Read failed error Num - Description
Explanation: Reading of the control file has failed. User Response: Correct the job stream and resubmit. System Action: Processing terminates.
`SXT7424I` | Input: ControlStatement
Explanation: The control statement has been read. System Action: Processing continues.
`SXT7425E` | null request error
Explanation: The control statement is blank. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7426E` | Request RequestToken invalid
Explanation: The request token is neither import nor export. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7427E` | Record type not given
Explanation: The control statement does not specify a record type. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7428E` | Record type Type is invalid
Explanation: The control statement contains an invalid record type. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7429E` | Record identifier not given
Explanation: The control statement does not contain a record identifier. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7430E` | Identifier RecordId too long
Explanation: The record identifier is invalid. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7431E` | Qualifier RecordQualifier is invalid
Explanation: The record qualifier in the control statement is invalid. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7432E` | Requested all types, but specified RecordId identifier
Explanation: The control statement is internally inconsistent. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7433E` | - Export trailer RC
Explanation: An error occurred during the writing process of the `export` trailer record. User Response: See the previous message. System Action: Processing terminates.
`SXT7434E` | - Export close error RC
Explanation: An error occurred during the closing of the configuration file. User Response: See the previous message. System Action: Processing terminates.
`SXT7437E` | Export request after import
Explanation: All control statements must be either import or export statements. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7438E` | Export open error RC
Explanation: An error occurred during the opening process of the configuration file. User Response: See the previous message. System Action: Processing terminates.
`SXT7440E` | Buffer Id not found
Explanation: An export request specifies the buffer Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7441E` | Message Id not found
Explanation: An export request specifies the message Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7442E` | Convert rule Id not found
Explanation: An export request specifies the convert rule Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7443E` | Back End System Id not found
Explanation: An export request specifies the backend system Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7444E` | Transport Id not found
Explanation: An export request specifies the transport Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7445E` | Recipe Id not found
Explanation: An export request specifies the recipe Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7446E` | Trigger Id not found
Explanation: An export request specifies the trigger Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7447E` | Group Id not found
Explanation: An export request specifies the Group Id, which does not exist. User Response: Correct and resubmit. System Action: Processing continues.
`SXT7448E` | Import request after export
Explanation: Import is currently not supported by this utility. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7449E` | Import open error RC
Explanation: An error occurred during the opening of the configuration file. User Response: See the previous message. System Action: Processing terminates.
`SXT7450C` | Cannot import in this utility
Explanation: Import is currently not supported by this utility. User Response: Use `SXT3CFUT` for import processing. System Action: Processing terminates.
`SXT7451I` | Use standard utility SXT3CFUT
Explanation: Import is not currently supported by this utility. User Response: Use `SXT3CFUT` for import processing. System Action: Processing terminates.
`SXT7452E` | Initialize failed
Explanation: The initialization process has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7453E` | Import or export init failed
Explanation: Common support initialization of import or export has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7454E` | Control file request was neither import nor export
Explanation: A control-statement error has occurred. User Response: Correct and resubmit. System Action: Processing terminates.
`SXT7455E` | Export trailer failed
Explanation: A write of the export trailer has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7456E` | Import interface term failed
Explanation: Common support termination of import or export has failed. User Response: See the previous message. System Action: Processing terminates.
`SXT7458E` | Close of Config file failed
Explanation: The closing process of the configuration file has returned an error. User Response: See the previous messages for more details on the error. System Action: Processing terminates.
`SXT7460E` | Table Request-Code failed, rc=RC
Explanation: A request to the tabling support routine has returned the nonzero return code RC. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7464E` | Function Duplicate Export Command for Identifier RC:RC RSN:RSN
Explanation: The process detected there are duplicate commands for the same Identifier. Returned the nonzero return code RC. User Response: Correct the command and run again. System Action: Processing terminates.
`SXT7502E` | Overflow st=Address, last= Address, len=Num
Explanation: The available workspace in the Linear Data Set has been exhausted. User Response: Terminate the current processing, reinitialize the environment, and reprocess those updates that were lost. If you get this error when doing the import operation to a blank new configuration file, add the "-Exxxxx" parameter to your import EXEC statement PARM parameter, where the xxxxx is the extra number of slots to be added in the configuration file internally. Then rerun the import process again. Default is 500 slots. System Action: The system issues this message and awaits further action.
`SXT7503E` | Delblk - null Xblk
Explanation: An internal error has been detected by the `DeleteBlock` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7504E` | Delblk - null start block
Explanation: An internal error has been detected by the `DeleteBlock` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7505E` | delblk bad type ddd
Explanation: An internal error has been detected by the `DeleteBlock` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7506E` | DELBLK err Address, and Address type Type
Explanation: An internal error has been detected by the `DeleteBlock` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7507E` | is_dup_id bad type Type
Explanation: An internal error has been detected by the `IsDuplicateId` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7508E` | null pointer to Is_Block_Used
Explanation: An internal error has been detected by the `Is_Block_Used` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7509E` | null startb to Is_Block_Used
Explanation: An internal error has been detected by the `Is_Block_Used` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7510E` | null startb to Is_Block_Used
Explanation: An internal error has been detected by the `Is_Block_Used` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7511E` | is_blk_used invalid type Type
Explanation: An internal error has been detected by the `Is_Block_Used` routine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7512E` | Buf Type miss incode =Num
Explanation: The buffer code Num is not in the buffer type lookup table. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7514E` | Buf Type miss intext =Description
Explanation: The buffer description Description is not in the buffer type lookup table. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7515E` | RV Type miss incode =Num
Explanation: The Rendezvous field code Num is not in the Rendezvous type lookup table. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7516E` | RV Type miss intext = Description
Explanation: The Rendezvous field description Description is not in the Rendezvous type lookup table. User Response: Contact TIBCO Support. System Action: Processing continues.
`SXT7517E` | Invalid block type Num
Explanation: An internal error has been detected in the `New Block` subroutine. User Response: Contact TIBCO Support. System Action: Processing terminates.
`SXT7589W` | Is_Blk_Used strange type
Explanation: The block type shown is not normally used in the current operation. System Action: Processing continues.
`SXT7802E` | Logger failed to start
Explanation: The routine to print messages cannot start and the program will terminate. User Response: Ensure that the DD statements TIBLOG and LOGDEBUG are in the job step. System Action: The program terminates.
`SXT9999C` | ALERT!!! <control block>
Explanation: A critical error has been discovered. User Response: Recycle Substation ES. System Action: Processing continues.

Copyright © TIBCO Software Inc. All rights reserved.