# Main Entry Panel

Substation ES Main Entry Panel provides the main entry to access the Transformer Configuration panels.

To access Substation ES the Transformer Configuration panels, perform the following steps:

1. Go to the ISPF Command Shell (Option 6).
2. Enter the `ex ’USERHLQ.CLIST(SXGSSPNL)’` command.

   where `USERHLQ` is the High Level Qualifier for your Substation ES installed libraries. Then Main Entry Panel is displayed.

3. Type 1 in the Select option field, and then press Enter.
   The Transformer Configuration panel is displayed.
   Note: To see a panel ID, enter `PANELID` on the command line. You can use the PANELID command to toggle the display of panel IDs on and off.

## Panel Layout

    SXGMP001 ---------------- TIBCO Software Inc. -----------------------------------
                                Main Entry Panel                       2004/10/12
                                                                            09:49

         SSSS  u  u  b    ssss   tttt  aaaa  tttt iiii oooo nn  n
         SS    u  u  b    ss      tt   a  a   tt   ii  o  o nn  n
          S    u  u  bbbb  s      tt   aaaa   tt   ii  o  o n n n
           SS  u  u  b  b   ss    tt   a  a   tt   ii  o  o n  nn
         SSSS  uuuu  bbbb ssss    tt   a  a   tt  iiii oooo n  nn

                           ((    EEEE  SSSS   ))
                          ((     E     SS      ))
                          ((     EE     S      ))
                          ((     E       SS    ))
                            ((   EEEE  SSSS   ))

    Select option    ==>
           1   Configuration
           2   LTA Search and Display Facility
           3   System Logger Search and Display Facility
    ENTER = PROCEED   END PFKey = RETURN

## Field Description

The following table lists the fields in the Substation ES Main Entry Panel:

Field | Description
--- | ---
Select option | You can select a panel. Three options are available: Configuration: enter `1` to select this option, press Enter, and then the Transformer Configuration panel is displayed, where you can start configuring Substation ES transformer. For more information about this panel, see Transformer Configuration Panel. LTA Search and Display Facility: enter `2` to select this option, press Enter, and then the Log Viewer Panel is displayed. System Logger Search and Display Facility: enter `3` to select this option, press Enter, and then the System Logger's TIBCO Log Stream Viewer Panel is displayed.

Copyright © TIBCO Software Inc. All rights reserved.