# Features

This is an overview for the destination, formats, and debug file of the LTA Agents.

## Destination

You can route information recorded by the LTA Agents as a formatted print file or to a disk file defined in Substation ES. Make your selection by specifying the correct destination in the System Startup Parameters.

## Formatting

If you specify an Agent destination to print (`P`), the information can be formatted in one of the following manners:

- As a single line. Message entries that exceed 80 characters are truncated. For example:

      SXA2601I Console Command 'REFR,RID='SXC-DPL-COBOL-START-TRAN-LONG-

- In full with additional identifying information, if available, for example:

      SXA2601I Console Command 'REFR,RID='SXC-DPL-COBOL-START-TRAN-LONG-NAME''

- In full with all the details available to the Agent. Normally, this format is for tracing information only. For example:

      009C 2011/05/05 15:31:14.6141 00000003 05002889 0 0 ID5: Mod: 66 Line: 180 Function: Flush_Admin_Buffer
       SXA2601I Console Command 'REFR,RID='SXC-DPL-COBOL-START-TRAN-LONG-NAME''

## Debug File

The Log and Trace Agents have their own debug file in which information is recorded with respect to their execution. The amount of information is determined by the value of the `LOGDBLVL` and `TRCDBLVL` keywords.

Note: Do not change the `LOGDBLVL` and `TRCDBLVL` value unless requested by a TIBCO representative. The content in the debug file is intended for TIBCO support and development staff only.
Copyright © TIBCO Software Inc. All rights reserved.