# Definitions

The following table shows a list of the user fields, whose names do not include the default prefix tibss-.

Field Name | Description
--- | ---
status | If a transformation, Substation ES, or BES error occurs, Substation ES adds the status field to the output message. Only one status field is added to a message. The value of the status field is incremented for each notification written to the `tibss-error-msg` message. In case of no errors, the status value is zero (0).
error-msg | This field is created if the appropriate Reply Method indicator has been set and if a transformation, Substation ES, or BES error is detected.
user field | This is the name of the field of a message defined to the Substation ES configuration that caused the transformation error. The content is a Substation ES descriptive and documented message.
error-info | This is a Substation ES warning or error informational field that is a Substation ES descriptive and documented message or a BES message.
ss-cfg-id | This is the current recipe or trigger identifier field and is always in a `tibss-error-msg` message.
ss-id | This is a Substation ES informational field that is always in a `tibss-error-msg` message.

Copyright © TIBCO Software Inc. All rights reserved.