# Single Message Values Panel

The Single Message Values panel displays the details of a log or trace record written to the log or trace disk file.

## Panel Layout

    SXLP004----------------- Single Message Values -------------------- Row 1 of 4
    Command ===>

     Msg Id: SXG1600I             Union id: 0               Stck: B9EC624552B80481
       Type: 154                      GRIN: 0                 RC: 0
       Date: 2003/08/25            Proc Id: 67111444      Reason: 0
       Time: 11:09:54.0919          Thread: 0

       Message-Dependent Values:
          Buffer length - 40
    -------------------------------------------------------------------------------
    |  No additional information
    |
    |  Message:
    |Log Agent Starting - Logging to TIBLOGF1
    ******************************* Bottom of data ********************************

## Field Description

The following table lists the fields in the Single Message Values panel:

Field | Description
--- | ---
Msg Id | An eight-character message identifier.
Type | The internal message type.
Date | The date that this message was recorded by Substation ES LTA Agent.
Time | The time that this message was recorded by Substation ES LTA Agent.
Union id | A representation of what message fields were recorded for this entry. See TIBCO Substation ES Messages and Codes for description.
GRIN | The internal Global Resource Identification Number.
Pro Id | The internal process identifier for identifying a Substation ES task or subtask.
Thread | The Substation ES thread that issues the message.
Stck | The internal 64-bit store clock value that uniquely identifies this message.
RC | The return code associated with the message.
Reason | The reason code associated with the message.
Buffer Length | A complete message description. If necessary, the message is displayed in multiple lines.

Copyright © TIBCO Software Inc. All rights reserved.