Open topic with navigation

TIBCO® Patterns 6.1.2

# Checking Server Status (lkt_svrnoop)

The server noop command literally does nothing. If the server is alive, it always returns success. This can be used to test connectivity.

    dvkerr_t lkt_svrnoop( lpar_t host);

## Input

## host (required)

For more information, see Communicating with TIBCO Patterns Servers.

Error codes and items returned by lkt_svrnoop

IPCERR | (none)
IPCTIMEOUT | (none)
IPCEOF | (none)
HANDSHAKE | (none)

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO® Patterns

Copyright © 2010-2025. Cloud Software Group, Inc. All Rights Reserved.