Open topic with navigation

TIBCO iProcess® Engine 11.10.0

# port_range_conf

The `port_range_conf` table defines the available port range configuration(s) for this iProcess Engine, for use with a firewall.

Note | In pre-10.4 iProcess Engine versions this information was defined in the `RNGMODE` parameter of the `SWDIR``\etc\staffcfg` file.

## Structure

The `port_range_conf` table has the following structure:

    TABLE port_range_conf (
    	port_range_id	integer		NOT NULL,
    	range_mode	smallint		NOT NULL,
    	range_size	integer		NOT NULL,
    	port_start	integer		NOT NULL,
    	rpc_start	integer		NOT NULL)

Column | Description
`port_range_id` | Unique ID of this particular port range configuration.
`range_mode` | Mode used by this port range configuration. One of the following values:
| • | `0` No Port or RPC ranging. A process uses the next available port number assigned by the operating system, and an RPC number based on the process ID.
| • | `1` Port ranging. A process uses a port number allocated from within the defined range, and an RPC number based on the process ID.
| • | `2` RPC ranging. A process uses the next available port number assigned by the operating system, and an RPC number allocated from within the defined range.
| • | `3` Port and RPC ranging. A process uses both a port number and an RPC number allocated from within the defined ranges.
`range_size` | The number of port and RPC numbers allowed in the port number and RPC number ranges.
`port_start` | The first number in the defined range of port numbers. (The last number = `port_start` + `range_size`.)
`rpc_start` | The first number in the defined range of RPC numbers. (The last number = `rpc_start` + `range_size`.)

## Primary Key

The following primary key is defined for this table.

Key Name | Column(s) | Index Tablespace
`pk_port_range_conf` | `port_range_id` | TINYINDEXSPACE

## Foreign Keys

None.

## Indexes

None.

## Storage

The following STORAGE values are defined for this table.

Value | Definition
Initial | TINYTABLESIZE
Percentage Increase | TINYTABLEPCTINCREASE
Tablespace | TINYTABLESPACE

## Table Activity

The `port_range_conf` table contains one row per defined port range configuration.

Rows are added, updated and deleted in the following situations.

A row is... | When...
added | a user defines a new port range configuration using the `SWDIR``\util\swadm` utility.
updated | a user changes an existing port range configuration, that is, either mode, range size or starting port/RPC number is changed, using the `SWDIR``\util\swadm` utility.
deleted | a user deletes an existing port range configuration using the `SWDIR``\util\swadm` utility.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO iProcess® Engine