Open topic with navigation

ibi™ Open Data Hub for Mainframe Connectors 1.0.8

# Usage Notes for Use of the zIIP Processor

- Maximize the blocksizes of data sources that are read or written by the server to reduce the number of I/Os required to access the file. This will reduce the number of switches to non-zIIP mode that the server agents have to make, thus permitting a greater percentage of zIIP contribution to the request.
- Move or rewrite functions developed at your site since the server must switch to non-zIIP mode for each call to such routines. You may be able to use one of the following possible solutions:
  - Move the routines from DEFINEs to COMPUTEs to reduce the number of times they are referenced. This tactic must be applied carefully, and only when report results would not change.
  - Rewrite the routines using DEFINE FUNCTION, which executes on the zIIP processor.
  - Confine the routine to a pre-step run with ZIIP=OFF which collects its calculated results, then use those calculations in the next step with ZIIP=ON.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

ibi™ Open Data Hub for Mainframe Connectors

Copyright © 2021-2025. Cloud Software Group, Inc. All Rights Reserved.