Open topic with navigation

TIBCO Rendezvous® 8.8.0

# Interpreting Log Output

Each line in the log file describes a significant event in the operation of a routing daemon. A time stamp indicates the date and time of the interaction. The remainder of the line is a string describing the event.

The log file begins with events in the routing daemon’s start sequence. First, it discovers its hardware and software operating environment:

    TIB/Rendezvous daemon
    Copyright 1994-2004 by TIBCO Software Inc.
    All rights reserved.
    Version 7.3.0
    2004-09-08 14:03:13 rvrd: Hostname: optimist
    2004-09-08 14:03:13 rvrd: Hostname IP address: 10.101.2.140
    2004-09-08 14:03:13 rvrd: Detected IP interface: 127.0.0.1 (lo)
    2004-09-08 14:03:13 rvrd: Detected IP interface: 10.101.2.140 (eth0)
    2004-09-08 14:03:13 rvrd: Using ticket file /usr/local/tibco/bin/tibrv.tkt
    2004-09-08 14:03:13 rvrd: Using store file /tmp/1.admin
    2004-09-08 14:03:13 rvrd: Warning: zlib compression not supported in SSL initialization.
    2004-09-08 14:03:13 rvrd: OpenSSL 0.9.7c 30 Sep 2003
    2004-09-08 14:03:13 rvrd: Initializing random pool...
    2004-09-08 14:03:13 rvrd: Invoking callback for case 2 and certificate 1.

Next, the routing daemon reads its configuration from its store file. In this example, it defines a router (routing table entry) named `optimist`. That router has an accept any neighbor interface, and a local network interface.

    2004-09-08 14:03:13 rvrd: [optimist]: Defined.
    2004-09-08 14:03:13 rvrd: [optimist]: Any neighbor is allowed to connect to local port 9666. Link cost: 1.
    2004-09-08 14:03:13 rvrd: [optimist]: Local network 7505.RV.TIBCO defined. Interface: 10.101.2.140. Service UDP port: 7505, Service spec: 7505, Network spec: 10.101.2. Link cost: 1.

The routing daemon finishes its start sequence by reporting the URL bindings of its browser administration interfaces.

    2004-09-08 14:03:13 rvrd: Http interface - http://optimist.rv.tibco.com:8000/

The administrator sets the logging parameters for normal activity.

    2004-09-08 14:08:35 rvrd: Logging: [Connections - On], [Subject Interest - On], [Subject Data - On].

Now the routing daemon begins normal operations. Log items reflect neighbor connections to other routers (`viggen-r1`), exchange of subscription interest information, and forwarding of message data.

    2004-09-08 14:13:26 rvrd: [optimist]: Connected to viggen-r1.
    2004-09-08 14:15:40 rvrd: [optimist]: Sending subscription for [TEST] to viggen-r1 for source 0A65023F/hpux11-viggen-n1.
    2004-09-08 14:16:30 rvrd: [optimist]: Received data on [TEST] from neighbor viggen-r1.
    2004-09-08 14:18:03 rvrd: [optimist]: Sending cancel for [TEST] to viggen-r1 for source 0A65023F/hpux11-viggen-n1.
    2004-09-08 14:19:31 rvrd: [optimist]: Disconnected from viggen-r1 (4).

Then `optimist` discovers another routing daemon (fanox) serving the same local network and service (redundancy for fault tolerance). Then it loses contact with fanox.

    2004-09-08 14:23:16 rvrd: [optimist]: Found fanox in 7505.RV.TIBCO.
    2004-09-08 14:24:24 rvrd: [optimist]: Lost fanox in 7505.RV.TIBCO.

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.