Open topic with navigation

TIBCO Rendezvous® 8.8.0

# tibrvMsg_GetCMTimeLimit()

Function

## Declaration

    tibrv_status tibrvMsg_GetCMTimeLimit(
        tibrvMsg         message,
        tibrv_f64*       timeLimit);

## Purpose

Extract the message time limit from a certified message.

## Remarks

Programs can explicitly set the message time limit (see tibrvMsg_SetCMTimeLimit()).

Zero is a special value, indicating no time limit.

If a time limit is not set for a message, this function returns the status code TIBRV_NOT_FOUND. This situation can occur only for unsent outbound messages, and for inbound unlabeled messages.

Time limits represent the minimum time that certified delivery is in effect.

This value represents the total time limit of the message, not the time remaining.

Parameter | Description
`message` | Extract the time limit from this message.
`timeLimit` | The program supplies a location. The function stores the time limit in that location.

## See Also

tibrvcmTransport_Send()

tibrvMsg_SetCMTimeLimit()

Did you find this helpful?

Yes No
Great!
Thanks for taking the time to give us some feedback.
Sorry about that

Why wasn't this helpful? (check all that apply)

Could not find what I was looking for
Instructions confusing or unclear
Instructions did not work

Want to tell us more?

Please select at least one option or provide details about the issue!!

Error occurred while submitting feedback.

Error2 occurred while submitting feedback.

TIBCO Rendezvous®

Copyright © 1997-2025. Cloud Software Group, Inc. All Rights Reserved.